; Adapter.INF  -- This file contains descriptions of all adapters 
;	supported in Chicago. Some adapters, like SCSI Adapters are
;	contained in their own INF.
;
;*** Created 10/6/93  (Creation Date)
; Mass Storage Adapters
;  *PNPA02B	Sony CD ROM Adapter            				Added

[Version]
signature="$CHICAGO$"
Class=Adapter
Provider=%Msft%
LayoutFile=LAYOUT.INF

; Class Install
[ClassInstall]
Addreg=AdapterReg

[AdapterReg]
HKR,,,,%AdapterClassName%


; Table of Contents
[Manufacturer]
%Sony%=Sony

[Sony]
%*pnpA02B.DeviceDesc%=SonyP,*pnpA02B


;********************************** Sony Driver Installation Sections
;
[SonyP]
LogConfig=SLCD1,SLCD2,SLCD3,SLCD4
CopyFiles=@SLCD32.mpd
AddReg=IOS,SonyRegLines

[SonyRegLines]
HKR,,PortDriver,,SLCD32.mpd



; HARDWARE SECTIONS
;******************************** Sony Hardware Sections
;
[*pnpA02B.Det]
LogConfig=SLCD1,SLCD2,SLCD3,SLCD4
AddReg=SonyReg2

[SLCD1]							; Pure PIO Configuration Factory default
ConfigPriority=HARDWIRED
IOConfig=1@320-340%3F0(3ff::),360-360(3ff::)

[SLCD2]							; IRQ in use
ConfigPriority=HARDWIRED
IOConfig=1@320-340%3F0(3ff::),360-360(3ff::)
IRQConfig=3,4,5,6

[SLCD3]							; DMA in use
ConfigPriority=HARDWIRED
IOConfig=1@320-340%3F0(3ff::),360-360(3ff::)
DMAConfig=1,2,3

[SLCD4]							; Both DMA and IRQ in use
ConfigPriority=HARDWIRED
IOConfig=1@320-340%3F0(3ff::),360-360(3ff::)
DMAConfig=1,2,3
IRQConfig=3,4,5,6

[SonyReg2]
HKR,,NoSetupUI,,1

;******************************** Common section
[IOS]
HKR,,DevLoader,,IOS.386

[DestinationDirs]
DefaultDestDir = 12             ; IOSubsys directory

[Strings]
Msft="Microsoft"
AdapterClassName="Adapter"
Sony="Sony Corp."
*pnpA02B.DeviceDesc="Sony Proprietary CD-Rom Controller"
